MOTOR DRIVER COMPARISON

|  |  |  |
| --- | --- | --- |
| Parameter | **L293d** | **L298n** |
| circuit | Quadruple half bridge | **Dual full H bridge** |
| Supply voltage range | 4.5-36v | **Upto 46 v** |
| Output current | 600 mA | **2 A** |
| Noise immunity | **High** | High |
| Over-temperature protection | NO | **YES** |
| Internal ESD protection | **YES** | NO |
| cost | **Low** | High |