Mass of robot = 1.5 KG

Radius of wheel = 5.5 cm = 0.055 m

Torque required = m\*g\*R

Where -

m= mass of robot

G= gravity

R=radius of wheel

Therefore

Torque = 1.5\*9.8\*0.055

=0.8085 N.M